Features
·  Network connected FFT processing system. 
·  Host system based on the Linux operating system for reliability and flexibility. 
·  Real-time data capture and processing. 
·  FPGA based re-configurable hardware based on the Xilinx Vertex-E series chips for fast and flexible signal processing. 
·  Parallel FFT, power and integration algorithms in hardware. 
·  Multiple processing engines per system. 
·  Processing engines can be interconnected with high speed connections. 
·  Alternative data processing algorithms can be developed and downloaded to the processing engines. 
·  GUI control application for configuration and control. 
·  Remote control by remote software. 
·  Data stored on local disk accessible via NFS, SMB, FTP or HTTP network protocols.