Some possible customisations
•	More FFT engines
•	50 MHz bandwidth in quadrature fft mode
•	Interconnection between processors to make real-time cross spectra